
**fluid pipe st37 mild steel seamless steel pipe**



http://img1.cdn.tradew.com/Y201701M1571336T6G6338481/W0H0/.jpg


**fluid pipe st37 mild steel seamless steel pipe**

|  |  |
| --- | --- |
| Name | api 5lb seamless steel pipe |
| Standard | ASTM A554, A249, A269 and A270, A312 |
| Thickness | 0.3mm to 300mm ( Tolerance +/- 0.02mm ) |
| Outer Diameter | 6mm to 159mm ( Tolerance +/- 0.02mm ) |
| Length | 6m or as customers' request ( Tolerance +/- 5mm ) |
| Application | Petroleum,Chemical enterprise, superheater of boiler, heat exchanger |

http://img1.cdn.tradew.com/Y201701M1571336T6G6338491/W0H0/.jpg







http://img1.cdn.tradew.com/Y201701M1571336T6G6338494/W0H0/.jpg



http://img1.cdn.tradew.com/Y201701M1571336T6G6338506/W0H0/.jpg



http://img1.cdn.tradew.com/Y201701M1571336T6G6338508/W0H0/.jpg

